badge_type=A


Broadcast: : STATUS 
admin 10,8,0,4,4/mod A/flatctrl useradmin/carryd  eat: carrot/
Client 1 Sent: 28  SETSTUFFDATA //DOOROPEN/TRUE10  LOOKTO 8 3
Client 1 Sent: 22  CarryDrink eat: carrot

Client 1 Sent: Sign 14
Client 1 Sent: Sign 1

Server Sent 1 : SYSTEMBROADCAST
¡Gracias por usar Servidor Old Davinci V2!



If IsNumeric(BadgeType(username(index))) = True Then
	SendData index, "YOUARECONTROLLER "
Status(index) = Status(index) & "mod " & BadgeType(username(index)) & "/flatctrl useradmin/"
Else
	SendData index, "YOUAREOWNER "
	Status(index) = Status(index) & "mod " & BadgeType(username(index)) & "/flatctrl useradmin/"
End If




Server is listening on port: 37120
A new Client with ID 1 and IP 127.0.0.1 connected!
Server Sent 1 : SECRET_KEY 
1337
Client 1 Sent: KEYENCRYPTED 3
Client 1 Sent: CLIENTIP MacromediaSecretIPAddressCookie: bd8e53e42066987ac942e9f961
Client 1 Sent: LOGIN admin admin
Server Sent 1 : SYSTEMBROADCAST
¡Gracias por usar Servidor Old Davinci V2!
Client 1 Sent: MESSENGERINIT
Client 1 Sent: UNIQUEMACHINEID 1003804292030220131108
Client 1 Sent: STAT /ShockwaveVersion/10.4.1
Client 1 Sent: INFORETRIEVE admin admin
Server Sent 1 : USEROBJECT
name=admin
email=admin@admin.admin
figure=sd=001/0&hr=001/255,255,255&hd=002/255,204,153&ey=001/0&fc=001/255,204,153&bd=001/255,204,153&lh=001/255,204,153&rh=001/255,204,153&ch=001/232,177,55&ls=001/232,177,55&rs=001/232,177,55&lg=001/119,159,187&sh=001/175,220,223
birthday=30.12.2010
phonenumber=+44
customData=Hi :D
had_read_agreement=1
sex=Male
country=
has_special_rights=1
badge_type=A






  if flatadmin = true then
    afs="flatctrl useradmin/"
  else
    afs = ""
  end if
  if GetVal(username,"admin") = "1" then
    afs = afs + "mod " + GetVal(username,"badge_type") + "/"
  end if

SocketSend ("STATUS " + chr(13) + Name + " " + parts(0) + "," + parts(1) + ",0," + parts(3) + "," + parts(3) + "/" + afs)





      case "GOAWAY"
        me.close
        Broadcast (room,"LOGOUT" + chr(13) + username)
      End Select

